This document has instructions on how to make modifications to the files included in mtemot.zip available for download in the file library of Trainsim.com. These modifications include animating both pantographs on two pantograph units and creating a duplicate set of files that have pantographs lowered to 6.2 meters.

WARNING: BACKUP ALL FILES BEFORE DOING ANY EDITS!!

The following is intended for those who already have some knowledge of the files MSTS uses and how to modify them.

NOTE: You should complete the edits in sequence as subsequent instructions may depend on previously completed edits.

NOTE: To perform the edits to shape (.s) files you will need to decompress them. I find Zipper ideal for this purpose. Don't forget to recompress the files when you are finished.

NOTE: Find the indicated line(s) and replace the underlined value(s) with value(s) in red.

NOTE: Microsoft's Wordpad text editor was used to make these edits and Paul Gausden's Shape Viewer (sview22.zip) was used to confirm the results.

NOTE: These edits are for personal use only and the modified files can not be distributed to others without the express permission of the files ORIGINAL authors.
______________________________________________________________________________________________
1-COSMETIC EDITS

MtE_B1_5A.s and MtE_B1_5B.s: This edit increases the volume sphere so that when the file is loaded into Shape Viewer it will display the entire model with the pantograph is raised.

	volumes ( 1 
			vol_sphere ( 
				vector ( 4.98516E-05 2.24161 0.288798 ) 4.8764 6

This edit moves the pantograph elements slightly towards the front of the model (when in the lowered position). This eliminates the sudden jerk that occurs when raising and lowering the pantograph.

	matrix PantographBottom1A ( 1 0 0 0 1 0 0 0 1 0 0.0609603 -0.901294 -0.6096 ) 
	matrix PantographBottom1B ( 1 0 0 0 1 0 0 0 1 0 0.0609603 0.317906 0.6096 ) 
	matrix PantographMiddle1A ( 1 0 0 0 1 0 0 0 1 0 0.21336 -2.79867 -2.506976 ) 
	matrix PantographMiddle1B ( 1 0 0 0 1 0 0 0 1 0 0.21336 2.21529 2.506984 ) 
	matrix PantographTop1A ( 1 0 0 0 1 0 0 0 1 0 0.44196 -0.291694 0 )
______________________________________________________________________________________________
2-ANIMATING SECOND PANTOGRAPH

MtE_MotorCar41.s:

	matrix FPantographBottom1A PantographBottom2A ( 1 0 0 0 1 0 0 0 1 0.0006096 0.140208 -0.572133 ) 
	matrix FPantographBottom1B PantographBottom2B ( 1 0 0 0 1 0 0 0 1 0 0.140208 0.575439 ) 
	matrix FPantographMiddle1A PantographMiddle2A ( 1 0 0 0 1 0 0 0 1 0 0.238963 -2.46768 ) 
	matrix FPantographMiddle1B PantographMiddle2B ( 1 0 0 0 1 0 0 0 1 0 0.238049 2.46002 ) 
	matrix FPantographTop1A PantographTop2A ( 1 0 0 0 1 0 0 0 1 0 0.382219 -0.00490046 ) 

	prim_state FPantographBottom1A_SolidNorm PantographBottom2A_SolidNorm ( 00000000 0 
		tex_idxs ( 1 0 ) 0 15 0 0 1 ) 
	prim_state FPantographBottom1B_SolidNorm PantographBottom2B_SolidNorm ( 00000000 0 
		tex_idxs ( 1 0 ) 0 16 0 0 1 ) 
	prim_state FPantographMiddle1A_SolidNorm PantographMiddle2A_SolidNorm ( 00000000 0 
		tex_idxs ( 1 0 ) 0 17 0 0 1 ) 
	prim_state FPantographMiddle1B_SolidNorm PantographMiddle2B_SolidNorm ( 00000000 0 
		tex_idxs ( 1 0 ) 0 18 0 0 1 ) 
	prim_state FPantographTop1A_SolidNorm PantographTop2A_SolidNorm ( 00000000 0 
		tex_idxs ( 1 0 ) 0 19 0 0 1 ) 

	anim_node FPantographBottom1A PantographBottom2A ( 
		controllers ( 0 1 
			tcb_rot ( 2 
				tcb_key ( 0 0 0 0 1 0 0 0 0 0 ) 
				tcb_key ( 1 -0.358368 0 0 0.93358 0 0 0 0 0 ) 
			) 
		) 
	) 
	anim_node FPantographBottom1B PantographBottom2B ( 
		controllers ( 0 1 
			tcb_rot ( 2 
				tcb_key ( 0 -6.98132E-08 0 0 1 0 0 0 0 0 ) 
				tcb_key ( 1 -0.358368 0 0 -0.93358 0 0 0 0 0 ) 
			)  
		) 
	) 
	anim_node FPantographMiddle1A PantographMiddle2A ( 
		controllers ( 0 2 
			tcb_rot ( 2 
				tcb_key ( 0 -4.01426E-07 0 0 1 0 0 0 0 0 ) 
				tcb_key ( 1 -0.313164 0 0 -0.949699 0 0 0 0 0 ) 
			) 
			linear_pos ( 2 
				linear_key ( 0 0 0.237744 -2.46278 ) 
				linear_key ( 1 0 1.47828 -1.90805 ) 
			) 
		) 
	) 
	anim_node FPantographMiddle1B PantographMiddle2B ( 
		controllers ( 0 2 
			tcb_rot ( 2 
				tcb_key ( 0 3.04616E-10 0.00436331 -6.98125E-08 0.99999 0 0 0 0 0 ) 
				tcb_key ( 1 -0.313164 0 0 0.949699 0 0 0 0 0 ) 
			) 
			linear_pos ( 2 
				linear_key ( 0 0 0.237744 2.46278 ) 
				linear_key ( 1 0 1.47828 1.90805 ) 
			) 
		) 
	) 
	anim_node FPantographTop1A PantographTop2A ( 
		controllers ( 0 1 
			linear_pos ( 2 
				linear_key ( 0 0 0.382219 0 ) 
				linear_key ( 1 0 3.05836 0 ) 
			) 
		) 
	) 
-----------------------------------------------------------------------------------------------------------------------------------------------------------
MtE_MotorCar42.s, MtE_MotorCar43.s: (Note: these units are set up to operate at the rear of a consist in "flipped" position.)

	matrix RPantographBottom1A PantographBottom2A ( 1 0 0 0 1 0 0 0 1 0.0006096 0.140208 -0.57211 ) 
	matrix RPantographBottom1B PantographBottom2B ( 1 0 0 0 1 0 0 0 1 0 0.140208 0.575462 ) 
	matrix RPantographMiddle1A PantographMiddle2A ( 1 0 0 0 1 0 0 0 1 0 0.238963 -2.46766 ) 
	matrix RPantographMiddle1B PantographMiddle2B ( 1 0 0 0 1 0 0 0 1 0 0.238049 2.46004 ) 
	matrix RPantographTop1A PantographTop2A ( 1 0 0 0 1 0 0 0 1 0 0.382219 -0.00487709 ) 

	prim_state RPantographBottom1A_SolidNorm PantographBottom2A_SolidNorm ( 00000000 0 
		tex_idxs ( 1 0 ) 0 15 0 0 1 ) 
	prim_state RPantographBottom1B_SolidNorm PantographBottom2B_SolidNorm ( 00000000 0 
		tex_idxs ( 1 0 ) 0 16 0 0 1 ) 
	prim_state RPantographMiddle1A_SolidNorm PantographMiddle2A_SolidNorm ( 00000000 0 
		tex_idxs ( 1 0 ) 0 17 0 0 1 ) 
	prim_state RPantographMiddle1B_SolidNorm PantographMiddle2B_SolidNorm ( 00000000 0 
		tex_idxs ( 1 0 ) 0 18 0 0 1 ) 
	prim_state RPantographTop1A_SolidNorm PantographTop2A_SolidNorm ( 00000000 0 
		tex_idxs ( 1 0 ) 0 19 0 0 1 ) 

	anim_node RPantographBottom1A PantographBottom2A ( 
		controllers ( 0 1 
			tcb_rot ( 2 
				tcb_key ( 0 0 0 0 1 0 0 0 0 0 ) 
				tcb_key ( 1 -0.358368 0 0 0.93358 0 0 0 0 0 ) 
			) 
		) 
	) 
	anim_node RPantographBottom1B PantographBottom2B ( 
		controllers ( 0 1 
			tcb_rot ( 2 
				tcb_key ( 0 -6.98132E-08 0 0 1 0 0 0 0 0 ) 
				tcb_key ( 1 -0.358368 0 0 -0.93358 0 0 0 0 0 ) 
			) 
		) 
	) 
	anim_node RPantographMiddle1A PantographMiddle2A ( 
		controllers ( 0 2 
			tcb_rot ( 2 
				tcb_key ( 0 -4.01426E-07 0 0 1 0 0 0 0 0 ) 
				tcb_key ( 1 -0.313164 0 0 -0.949699 0 0 0 0 0 ) 
			) 
			linear_pos ( 2 
				linear_key ( 0 0 0.237744 -2.46278 ) 
				linear_key ( 1 0 1.47828 -1.90805 ) 
			) 
		) 
	) 
	anim_node RPantographMiddle1B PantographMiddle2B ( 
		controllers ( 0 2 
			tcb_rot ( 2 
				tcb_key ( 0 3.04616E-10 0.00436331 -6.98125E-08 0.99999 0 0 0 0 0 ) 
				tcb_key ( 1 -0.313164 0 0 0.949699 0 0 0 0 0 ) 
			) 
			linear_pos ( 2 
				linear_key ( 0 0 0.237744 2.46278 ) 
				linear_key ( 1 0 1.47828 1.90805 ) 
			) 
		) 
	) 
	anim_node RPantographTop1A PantographTop2A ( 
		controllers ( 0 1 
			linear_pos ( 2 
				linear_key ( 0 0 0.382219 0 ) 
				linear_key ( 1 0 3.05836 0 ) 
			) 
		) 
	) 
-----------------------------------------------------------------------------------------------------------------------------------------------------------
Mte_P1_6.s, Mte_P1_7.s, Mte_P1_8.s, Mte_P1_9.s: Animation nodes for second pantograph were not finished on these models.
-----------------------------------------------------------------------------------------------------------------------------------------------------------
Mte_P5_3.s:

	matrix PantographBottom1AF PantographBottom2A ( 1 0 0 0 1 0 0 0 1 0 0.0609603 -0.6096 ) 
	matrix PantographBottom1BF PantographBottom2B ( 1 0 0 0 1 0 0 0 1 0 0.0609603 0.6096 ) 
	matrix PantographMiddle1AF PantographMiddle2A ( 1 0 0 0 1 0 0 0 1 0 0.21336 -2.50698 ) 
	matrix PantographMiddle1BF PantographMiddle2B ( 1 0 0 0 1 0 0 0 1 0 0.21336 2.50698 ) 
	matrix PantographTop1AF PantographTop2A ( 1 0 0 0 1 0 0 0 1 0 0.44196 0 ) 

	prim_state PantographBottom1AF_SolidNorm PantographBottom2A_SolidNorm ( 00000000 0 
		tex_idxs ( 1 1 ) 0 6 0 0 1 ) 
	prim_state PantographBottom1BF_SolidNorm PantographBottom2B_SolidNorm ( 00000000 0 
		tex_idxs ( 1 1 ) 0 7 0 0 1 ) 
	prim_state PantographMiddle1AF_SolidNorm PantographMiddle2A_SolidNorm ( 00000000 0 
		tex_idxs ( 1 1 ) 0 8 0 0 1 ) 
	prim_state PantographMiddle1BF_SolidNorm PantographMiddle2B_SolidNorm ( 00000000 0 
		tex_idxs ( 1 1 ) 0 9 0 0 1 ) 
	prim_state PantographTop1AF_SolidNorm PantographTop2A_SolidNorm ( 00000000 0 
		tex_idxs ( 1 1 ) 0 10 0 0 1 ) 

	anim_node PantographBottom1AF PantographBottom2A ( 
		controllers ( 0 1 
			tcb_rot ( 2 
				tcb_key ( 0 0 0 0 1 0 0 0 0 0 ) 
				tcb_key ( 8 -0.333807 0 0 0.942641 0 0 0 0 0 ) 
			) 
		) 
	) 
	anim_node PantographBottom1BF PantographBottom2B ( 
		controllers ( 0 1 
			tcb_rot ( 2 
				tcb_key ( 0 0 0 0 1 0 0 0 0 0 ) 
				tcb_key ( 8 -0.333807 0 0 -0.942642 0 0 0 0 0 ) 
			) 
		) 
	) 
	anim_node PantographMiddle1AF PantographMiddle2A ( 
		controllers ( 0 2 
			tcb_rot ( 2 
				tcb_key ( 0 0 0 0 1 0 0 0 0 0 ) 
				tcb_key ( 8 -0.284015 0 0 -0.95882 0 0 0 0 0 ) 
			) 
			linear_pos ( 2 
				linear_key ( 0 0 0.21336 -2.50698 ) 
				linear_key ( 8 0 1.35941 -1.9873 ) 
			) 
		) 
	) 
	anim_node PantographMiddle1BF PantographMiddle2B ( 
		controllers ( 0 2 
			tcb_rot ( 2 
				tcb_key ( 0 0 0 0 1 0 0 0 0 0 ) 
				tcb_key ( 8 -0.284015 0 0 0.95882 0 0 0 0 0 ) 
			) 
			linear_pos ( 2 
				linear_key ( 0 0 0.21336 2.50698 ) 
				linear_key ( 8 0 1.35941 1.9873 ) 
			) 
		) 
	) 
	anim_node PantographTop1AF PantographTop2A ( 
		controllers ( 0 1 
			linear_pos ( 2 
				linear_key ( 0 0 0.44196 0 ) 
				linear_key ( 8 0 2.88036 0 ) 
			) 
		) 
	) 

-----------------------------------------------------------------------------------------------------------------------------------------------------------
Mte_P5_4.s:

	matrix PantographBottom1AF PantographBottom1A ( 1 0 0 0 1 0 0 0 1 0 0.0609603 -0.6096 ) 
	matrix PantographBottom1BF PantographBottom1B ( 1 0 0 0 1 0 0 0 1 0 0.0609603 0.6096 ) 
	matrix PantographMiddle1AF PantographMiddle1A ( 1 0 0 0 1 0 0 0 1 0 0.21336 -2.50698 ) 
	matrix PantographMiddle1BF PantographMiddle1B ( 1 0 0 0 1 0 0 0 1 0 0.21336 2.50698 ) 
	matrix PantographTop1AF PantographTop1AF ( 1 0 0 0 1 0 0 0 1 0 0.44196 0 ) 
	matrix Mount ( 1 0 0 0 1 0 0 0 1 0 4.02336 5.0292 ) 
	matrix PantographBottom1A PantographBottom2A ( 1 0 0 0 1 0 0 0 1 0 0.0609603 -0.6096 ) 
	matrix PantographBottom1B PantographBottom2B ( 1 0 0 0 1 0 0 0 1 0 0.0609603 0.6096 ) 
	matrix PantographMiddle1B PantographMiddle2B ( 1 0 0 0 1 0 0 0 1 0 0.21336 2.50698 ) 
	matrix PantographMiddle1A PantographMiddle2A ( 1 0 0 0 1 0 0 0 1 0 0.21336 -2.50698 ) 
	matrix PantographTop1A PantographTop2A ( 1 0 0 0 1 0 0 0 1 0 0.44196 0 )

	prim_state PantographBottom1AF_SolidNorm PantographBottom1A_SolidNorm ( 00000000 0 
		tex_idxs ( 1 1 ) 0 6 0 0 1 ) 
	prim_state PantographBottom1BF_SolidNorm PantographBottom1B_SolidNorm ( 00000000 0 
		tex_idxs ( 1 1 ) 0 7 0 0 1 ) 
	prim_state PantographMiddle1AF_SolidNorm PantographMiddle1A_SolidNorm ( 00000000 0 
		tex_idxs ( 1 1 ) 0 8 0 0 1 ) 
	prim_state PantographMiddle1BF_SolidNorm PantographMiddle1B_SolidNorm ( 00000000 0 
		tex_idxs ( 1 1 ) 0 9 0 0 1 ) 
	prim_state PantographTop1AF_SolidNorm PantographTop1A_SolidNorm ( 00000000 0 
		tex_idxs ( 1 1 ) 0 10 0 0 1 ) 
	prim_state Mount_SolidNorm ( 00000000 0 
		tex_idxs ( 1 1 ) 0 11 0 0 1 ) 
	prim_state PantographBottom1A_SolidNorm PantographBottom2A_SolidNorm ( 00000000 0 
		tex_idxs ( 1 1 ) 0 12 0 0 1 ) 
	prim_state PantographBottom1B_SolidNorm PantographBottom2B_SolidNorm ( 00000000 0 
		tex_idxs ( 1 1 ) 0 13 0 0 1 ) 
	prim_state PantographMiddle1B_SolidNorm PantographMiddle2B_SolidNorm ( 00000000 0 
		tex_idxs ( 1 1 ) 0 14 0 0 1 ) 
	prim_state PantographMiddle1A_SolidNorm PantographMiddle2A_SolidNorm ( 00000000 0 
		tex_idxs ( 1 1 ) 0 15 0 0 1 ) 
	prim_state PantographTop1A_SolidNorm PantographTop2A_SolidNorm ( 00000000 0 
		tex_idxs ( 1 1 ) 0 16 0 0 1 ) 
 
	anim_node PantographBottom1AF PantographBottom1A ( 
		controllers ( 0 1 
			tcb_rot ( 2 
				tcb_key ( 0 0 0 0 1 0 0 0 0 0 ) 
				tcb_key ( 8 -0.333807 0 0 0.942641 0 0 0 0 0 ) 
			) 
		) 
	) 
	anim_node PantographBottom1BF PantographBottom1B ( 
		controllers ( 0 1 
			tcb_rot ( 2 
				tcb_key ( 0 0 0 0 1 0 0 0 0 0 ) 
				tcb_key ( 8 -0.333807 0 0 -0.942642 0 0 0 0 0 ) 
			) 
		) 
	) 
	anim_node PantographMiddle1AF PantographMiddle1A ( 
		controllers ( 0 2 
			tcb_rot ( 2 
				tcb_key ( 0 0 0 0 1 0 0 0 0 0 ) 
				tcb_key ( 8 -0.284015 0 0 -0.95882 0 0 0 0 0 ) 
			) 
			linear_pos ( 2 
				linear_key ( 0 0 0.21336 -2.50698 ) 
				linear_key ( 8 0 1.35941 -1.9873 ) 
			) 
		) 
	) 
	anim_node PantographMiddle1BF PantographMiddle1B ( 
		controllers ( 0 2 
			tcb_rot ( 2 
				tcb_key ( 0 0 0 0 1 0 0 0 0 0 ) 
				tcb_key ( 8 -0.284015 0 0 0.95882 0 0 0 0 0 ) 
			) 
			linear_pos ( 2 
				linear_key ( 0 0 0.21336 2.50698 ) 
				linear_key ( 8 0 1.35941 1.9873 ) 
			) 
		) 
	) 
	anim_node PantographTop1AF PantographTop1A ( 
		controllers ( 0 1 
			linear_pos ( 2 
				linear_key ( 0 0 0.44196 0 ) 
				linear_key ( 8 0 2.88036 0 ) 
			) 
		) 
	) 
	anim_node Mount ( 
		controllers ( 0 
		) 
	) 
	anim_node PantographBottom1A PantographBottom2A ( 
		controllers ( 1 
			tcb_rot ( 2 
				tcb_key ( 0 0 0 0 1 0 0 0 0 0 ) 
				tcb_key ( 8 -0.333807 0 0 0.942641 0 0 0 0 0 ) 
			) 
		) 
	) 
	anim_node PantographBottom1B PantographBottom2B ( 
		controllers ( 1 
			tcb_rot ( 2 
				tcb_key ( 0 0 0 0 1 0 0 0 0 0 ) 
				tcb_key ( 8 -0.333807 0 0 -0.942642 0 0 0 0 0 ) 
			) 
		) 
	) 
	anim_node PantographMiddle1B PantographMiddle2B ( 
		controllers ( 2 
			tcb_rot ( 2 
				tcb_key ( 0 0 0 0 1 0 0 0 0 0 ) 
				tcb_key ( 8 -0.284015 0 0 0.95882 0 0 0 0 0 ) 
			) 
			linear_pos ( 2 
				linear_key ( 0 0 0.21336 2.50698 ) 
				linear_key ( 8 0 1.35941 1.9873 ) 
			) 
		) 
	) 
	anim_node PantographMiddle1A PantographMiddle2A ( 
		controllers ( 2 
			tcb_rot ( 2 
				tcb_key ( 0 0 0 0 1 0 0 0 0 0 ) 
				tcb_key ( 8 -0.284015 0 0 -0.95882 0 0 0 0 0 ) 
			) 
			linear_pos ( 2 
				linear_key ( 0 0 0.21336 -2.50698 ) 
				linear_key ( 8 0 1.35941 -1.9873 ) 
			) 
		) 
	) 
	anim_node PantographTop1A PantographTop2A ( 
		controllers ( 1 
			linear_pos ( 2 
				linear_key ( 0 0 0.44196 0 ) 
				linear_key ( 8 0 2.88036 0 ) 
			) 
		) 
	) 

______________________________________________________________________________________________
3-ADD CONTROL TO USE SECOND PANTOGRAPH

MtE_CabCar20.eng, MtE_CabCar21.eng, MtE_CabCar22.eng, MtE_CabCar24.eng, MtE_CabCar51.eng, MtE_CabCar52.eng, MtE_CabCar55.eng, MtE_MotorBaggage18.eng, MtE_MotorBaggage19.eng, MtE_MotorCar10.eng, MtE_MotorCar12.eng, MtE_MotorCar13.eng, MtE_MotorCar14.eng, MtE_MotorCar15.eng, MtE_MotorCar41.eng, MtE_MotorCar42.eng, MtE_MotorCar43.eng, MtE_MotorCombine16.eng, MtE_MotorCombine17.eng, MtE_MotorWorks11.eng, Mte_P1_6.s, Mte_P1_7.s, Mte_P1_8.s, Mte_P1_9.s, MtE_P5_3eng, and MtE_P5_4.eng: These edits add a control so that the second pantograph can be raised and lowered on any two pantograph unit in the player consist. (Note: editing the last 1 to a zero will start the sim with the pantograph(s) lowered.)

	Vigilance ( 0 1 0 )
	PantographToggle1 ( 0 1 1 )
	PantographToggle2 ( 0 1 1 )
	Headlights ( 0 0.25 1 0 )

______________________________________________________________________________________________
4-CREATING UNITS WITH PANTOGRAPHS SET TO 6.2 METERS (the method used is described in a tutorial ("How To Adjust Your (Animated) Pantograph Height") by Paul Gausden on the Steam4Me website.)

Make copies of MtE_B1_5A.s and MtE_B1_5B.s rename them Mte_B1_5A-62m.s and MtE_B1_5B-62m.s respectively.

-----------------------------------------------------------------------------------------------------------------------------------------------------------
MtE_B1_5A-62m.s and MtE_B1_5B-62m.s:

	anim_node PantographBottom1A ( 
		controllers ( 2 
			tcb_rot ( 2 
				tcb_key ( 0 0 0 0 1 0 0 0 0 0 ) 
				tcb_key ( 8 -0.333807 -0.1736482 0 0 0.942641 0.9848078 0 0 0 0 0 ) 
			) 
			linear_pos ( 2 
				linear_key ( 0 0 0.06096 -0.6096 ) 
				linear_key ( 8 0 0.06096 -0.6096 ) 
			) 
		) 
	) 
	anim_node PantographBottom1B ( 
		controllers ( 2 
			tcb_rot ( 2 
				tcb_key ( 0 0 0 0 1 0 0 0 0 0 ) 
				tcb_key ( 8 -0.333807 -0.1736482 0 0 -0.942642 -0.9848078 0 0 0 0 0 ) 
			) 
			linear_pos ( 2 
				linear_key ( 0 0 0.06096 0.6096 ) 
				linear_key ( 8 0 0.06096 0.6096 ) 
			) 
		) 
	) 
	anim_node PantographMiddle1A ( 
		controllers ( 2 
			tcb_rot ( 2 
				tcb_key ( 0 0 0 0 1 0 0 0 0 0 ) 
				tcb_key ( 8 -0.284015 -0.1564345 0 0 -0.95882 -0.9876883 0 0 0 0 0 ) 
			) 
			linear_pos ( 2 
				linear_key ( 0 0 0.21336 -2.50698 ) 
				linear_key ( 8 0 1.35941 0.85 -1.9873 -2.35 ) 
			) 
		) 
	) 
	anim_node PantographMiddle1B ( 
		controllers ( 2 
			tcb_rot ( 2 
				tcb_key ( 0 0 0 0 1 0 0 0 0 0 ) 
				tcb_key ( 8 -0.284015 -0.1564345 0 0 0.95882 0.9876883 0 0 0 0 0 ) 
			) 
			linear_pos ( 2 
				linear_key ( 0 0 0.21336 2.50698 ) 
				linear_key ( 8 0 1.35941 0.85 1.9873 2.35 ) 
			) 
		) 
	) 
	anim_node PantographTop1A ( 
		controllers ( 1 
			linear_pos ( 2 
				linear_key ( 0 0 0.44196 0 ) 
				linear_key ( 8 0 2.88036 1.88036 0 ) 
			) 
		) 
	) 

-----------------------------------------------------------------------------------------------------------------------------------------------------------
Make copies of MtE_B1_5A.eng, MtE_B1_5A.sd, MtE_B1_5B.eng, and MtE_B1_5B.sd. Name the copies MtE_B1_5A-62m.eng, MtE_B1_5A-62m.sd, MtE_B1_5B-62m.eng, and MtE_B1_5B-62m.sd respectively.

-----------------------------------------------------------------------------------------------------------------------------------------------------------
MtE_B1_5A-62m.eng:

	Wagon ( MtE_B1_5A MtE_B1_5A-62m
		Type ( Engine )
		WagonShape ( MtE_B1_5A.s MtE_B1_5A-62m )
		Size  ( 3.20106m 4.49827m 9.5m )

	Engine ( MtE_B1_5A MtE_B1_5A-62m
		Wagon ( MtE_B1_5A MtE_B1_5A-62m
		Type ( Electric )
		MaxPower ( 425.2kW )

	Sound ( "LowPitch_P01235_cab.sms" )
	Name ( "MtE B1 Boxcab 5" "MtE B1 Boxcab 5 6.2meter" )
	Description (

-----------------------------------------------------------------------------------------------------------------------------------------------------------
MtE_B1_5A-62m.sd:

	SIMISA@@@@@@@@@@JINX0t1t______
	Shape ( MtE_B1_5A.s MtE_B1_5A-62m.s
		ESD_Detail_Level ( 0 )
		ESD_Software_DLev ( 3 )
		ESD_Alternative_Texture ( 0 )
		ESD_Bounding_Box ( -1.52 0.02 -4.55 1.52 4.48 4.55 )
	)

-----------------------------------------------------------------------------------------------------------------------------------------------------------
MtE_B1_5B-62m.eng:

	Wagon ( MtE_B1_5B MtE_B1_5B-62m
		Type ( Engine )
		WagonShape ( MtE_B1_5B.s MtE_B1_5B-62m )
		Size  ( 3.20106m 4.49827m 9.5m )

	Engine ( MtE_B1_5B MtE_B1_5B-62m
		Wagon ( MtE_B1_5B MtE_B1_5B-62m
		Type ( Electric )
		MaxPower ( 425.2kW )

	Sound ( "LowPitch_P01235_cab.sms" )
	Name ( "MtE B1 Boxcab 5 [B Unit]" "MtE B1 Boxcab 5 [B Unit] 6.2meter" )
	Description (

-----------------------------------------------------------------------------------------------------------------------------------------------------------
MtE_B1_5B-62m.sd:

	SIMISA@@@@@@@@@@JINX0t1t______
	Shape ( MtE_B1_5B.s MtE_B1_5B-62m.s
		ESD_Detail_Level ( 0 )
		ESD_Software_DLev ( 3 )
		ESD_Alternative_Texture ( 0 )
		ESD_Bounding_Box ( -1.52 0.02 -4.55 1.52 4.48 4.55 )
	)

-----------------------------------------------------------------------------------------------------------------------------------------------------------
Make copies of MtE_MotorBaggage18.s, MtE_MotorBaggage18.sd, MtE_MotorBaggage18.eng, MtE_MotorBaggage19.s, MtE_MotorBaggage19.sd, MtE_MotorBaggage19.eng, MtE_MotorCar10.s, MtE_Motorcar10.sd, MtE_MotorCar10.eng, MtE_MotorCar12.s, MtE_Motorcar12.sd, MtE_MotorCar12.eng, MtE_MotorCar13.s, MtE_Motorcar13.sd, MtE_MotorCar13.eng, MtE_MotorCar14.s, MtE_Motorcar14.sd, MtE_MotorCar14.eng, MtE_MotorCar15.s, MtE_Motorcar15.sd, MtE_MotorCar15.eng, MtE_MotorCombine16.s, MtE_MotorCombine16.sd, MtE_MotorCombine16eng, MtE_MotorCombine17.s, MtE_MotorCombine17.sd, MtE_MotorCombine17eng, MtE_MotorWorks11.s, MtE_MotorWorks11.sd, MtE_MotorWorks11.eng and name them MtE_MotorBaggage18-62m.s, MtE_MotorBaggage18-62m.sd, MtE_MotorBaggage18-62m.eng, MtE_MotorBaggage19-62m.s, MtE_MotorBaggage19-62m.sd, MtE_MotorBaggage19-62m.eng, MtE_MotorCar10-62m.s, MtE_Motorcar10-62m.sd, MtE_MotorCar10-62m.eng, MtE_MotorCar12-62m.s, MtE_Motorcar12-62m.sd, MtE_MotorCar12-62m.eng, MtE_MotorCar13-62m.s, MtE_Motorcar13-62m.sd, MtE_MotorCar13-62m.eng, MtE_MotorCar14-62m.s, MtE_Motorcar14-62m.sd, MtE_MotorCar14-62m.eng, MtE_MotorCar15-62m.s, MtE_Motorcar15-62m.sd, MtE_MotorCar15-62m.eng, MtE_MotorCombine16-62m.s, MtE_MotorCombine16-62m.sd, MtE_MotorCombine16-62m.eng, MtE_MotorCombine17-62m.s, MtE_MotorCombine17-62m.sd, MtE_MotorCombine17-62m.eng, MtE_MotorWorks11-62m.s, MtE_MotorWorks11-62m.sd, MtE_MotorWorks11-62m.eng respectively.

-----------------------------------------------------------------------------------------------------------------------------------------------------------
MtE_MotorBaggage18-62m.s, MtE_MotorBaggage19-62m.s, MtE_MotorCar10-62m.s, MtE_MotorCar12-62m.s, MtE_MotorCar13-62m.s, MtE_MotorCar14-62m.s, MtE_MotorCar15-62m.s, MtE_MotorCombine16-62m.s, MtE_MotorCombine17-62m.s, MtE_MotorWorks11-62m.s:

	anim_node PantographBottom1A ( 
		controllers ( 1 
			tcb_rot ( 2 
				tcb_key ( 0 0 0 0 1 0 0 0 0 0 ) 
				tcb_key ( 1 -0.358368 -0.190809 0 0 0.93358 0.9816272 0 0 0 0 0 ) 
			) 
		) 
	) 
	anim_node PantographBottom1B ( 
		controllers ( 1 
			tcb_rot ( 2 
				tcb_key ( 0 -6.98132E-08 0 0 1 0 0 0 0 0 ) 
				tcb_key ( 1 -0.358368 -0.190809 0 0 -0.93358 -0.9816272 0 0 0 0 0 ) 
			) 
		) 
	) 
	anim_node PantographMiddle1B ( 
		controllers ( 2 
			tcb_rot ( 2 
				tcb_key ( 0 3.04616E-10 0.00436331 -6.98125E-08 0.99999 0 0 0 0 0 ) 
				tcb_key ( 1 -0.313164 -0.190809 0 0 0.949699 0.9816272 0 0 0 0 0 ) 
			) 
			linear_pos ( 2 
				linear_key ( 0 0 0.323393 2.46492 ) 
				linear_key ( 1 -0.0036576 1.55852 1.049 1.9079 2.3 ) 
			) 
		) 
	) 
	anim_node PantographMiddle1A ( 
		controllers ( 2 
			tcb_rot ( 2 
				tcb_key ( 0 -4.01426E-07 0 0 1 0 0 0 0 0 ) 
				tcb_key ( 1 -0.313164 -0.190809 0 0 -0.949699 -0.9816272 0 0 0 0 0 ) 
			) 
			linear_pos ( 2 
				linear_key ( 0 0 0.324307 -2.46278 ) 
				linear_key ( 1 -0.000634289 1.56028 1.049 -1.90743 -2.3 ) 
			) 
		) 
	) 
	anim_node PantographTop1A ( 
		controllers ( 1 
			linear_pos ( 2 
				linear_key ( 0 -0.0006096 0.470095 -0.0027243 ) 
				linear_key ( 1 0.00158496 3.13554 2.13554 -0.00122377 ) 
			) 
		) 
	) 

-----------------------------------------------------------------------------------------------------------------------------------------------------------
MtE_MotorBaggage18-62m.sd:

Shape ( MtE_MotorBaggage18.s MtE_MotorBaggage18-62m.s
	ESD_Detail_Level ( 0 )
	ESD_Software_DLev ( 3 )
	ESD_Alternative_Texture ( 0 )
	ESD_Bounding_Box ( -1.512000 0.023000 -9.600000 1.512000 4.250000 9.600000 )
)

-----------------------------------------------------------------------------------------------------------------------------------------------------------
MtE_MotorBaggage18-62m.eng:

Wagon ( MtE_MotorBaggage18 MtE_MotorBaggage18-62m
	Type ( Engine )
	WagonShape ( MtE_MotorBaggage18.s MtE_MotorBaggage18-62m.s )
 	PassengerCapacity ( 1 )
	Size  ( 3.01992m 4.22469m 19.7m )

Engine ( MtE_MotorBaggage18 MtE_MotorBaggage18-62m
    Wagon ( MtE_MotorBaggage18 MtE_MotorBaggage18-62m )
    Type ( Electric )

Sound ( "MediumPitch_P01235_cab.sms" )
    Name ( "MtE Motor Baggage 18" "MtE Motor Baggage 18 6.2meter" )
    Description (

-----------------------------------------------------------------------------------------------------------------------------------------------------------
MtE_MotorBaggage19-62m.sd:

Shape ( MtE_MotorBaggage19.s MtE_MotorBaggage19-62m.s
	ESD_Detail_Level ( 0 )
	ESD_Software_DLev ( 3 )
	ESD_Alternative_Texture ( 0 )
	ESD_Bounding_Box ( -1.512000 0.023000 -9.600000 1.512000 4.250000 9.600000 )
)

-----------------------------------------------------------------------------------------------------------------------------------------------------------
MtE_MotorBaggage19-62m.eng:

Wagon ( MtE_MotorBaggage19 MtE_MotorBaggage19-62m
	Type ( Engine )
	WagonShape ( MtE_MotorBaggage19.s MtE_MotorBaggage19-62m.s )
 	PassengerCapacity ( 1 )
	Size  ( 3.01992m 4.22469m 19.7m )

Engine ( MtE_MotorBaggage19 MtE_MotorBaggage19-62m
    Wagon ( MtE_MotorBaggage19 MtE_MotorBaggage19-62m )
    Type ( Electric )

    Sound ( "MediumPitch_P01235_cab.sms" )
    Name ( "MtE Motor Baggage 19" "MtE Motor Baggage 19 6.2meter" )
    Description (

-----------------------------------------------------------------------------------------------------------------------------------------------------------
Shape ( MtE_MotorCar10.s MtE_MotorCar10-62m.s
	ESD_Detail_Level ( 0 )
	ESD_Software_DLev ( 3 )
	ESD_Alternative_Texture ( 0 )
	ESD_Bounding_Box ( -1.512000 0.023000 -9.600000 1.512000 4.250000 9.600000 )
)

-----------------------------------------------------------------------------------------------------------------------------------------------------------
MtE_MotorCar10-62m.eng:

Wagon ( MtE_MotorCar10 MtE_MotorCar10-62m
	Type ( Engine )
	WagonShape ( MtE_MotorCar10.s MtE_MotorCar10-62m.s )
 	PassengerCapacity ( 72.0 )
	Size  ( 3.01992m 4.22469m 19.7m )

Engine ( MtE_MotorCar10 MtE_MotorCar10-62m
    Wagon ( MtE_MotorCar10 MtE_MotorCar10-62m )
    Type ( Electric )

Sound ( "MediumPitch_P01235_cab.sms" )
Name ( "MtE Motor 10 [one panto/fwd]" "MtE Motor 10 [one panto/fwd] 6.2meter" )
Description (

-----------------------------------------------------------------------------------------------------------------------------------------------------------
MtE_Motorcar12-62m.sd:

Shape ( MtE_MotorCar12.s MtE_MotorCar12-62m.s
	ESD_Detail_Level ( 0 )
	ESD_Software_DLev ( 3 )
	ESD_Alternative_Texture ( 0 )
	ESD_Bounding_Box ( -1.512000 0.023000 -9.600000 1.512000 4.250000 9.600000 )
)

-----------------------------------------------------------------------------------------------------------------------------------------------------------
MtE_MotorCar12-62m.eng:

Wagon ( MtE_Motorcar12 MtE_Motorcar12-62m
	Type ( Engine )
	WagonShape ( MtE_Motorcar12.s )
 	PassengerCapacity ( 72.0 )
	Size  ( 3.01992m 4.22469m 19.7m )

Engine ( MtE_Motorcar12 MtE_Motorcar12-62m
    Wagon ( MtE_Motorcar12 MtE_Motorcar12-62m )
    Type ( Electric )

    Sound ( "MediumPitch_P01235_cab.sms" )
    Name ( "MtE Motor 12 [one panto/rear]" "MtE Motor 12 [one panto/rear] 6.2meter" )
    Description (

-----------------------------------------------------------------------------------------------------------------------------------------------------------
MtE_Motorcar13-62m.sd:

Shape ( MtE_MotorCar13.s MtE_MotorCar13-62m.s
	ESD_Detail_Level ( 0 )
	ESD_Software_DLev ( 3 )
	ESD_Alternative_Texture ( 0 )
	ESD_Bounding_Box ( -1.512000 0.023000 -9.600000 1.512000 4.250000 9.600000 )
)

-----------------------------------------------------------------------------------------------------------------------------------------------------------
MtE_MotorCar13-62m.eng:

Wagon ( MtE_MotorCar13 MtE_MotorCar13-62m
	Type ( Engine )
	WagonShape ( MtE_MotorCar13.s MtE_MotorCar13-62m.s )
 	PassengerCapacity ( 72.0 )
	Size  ( 3.01992m 4.22469m 19.7m )

Engine ( MtE_MotorCar13 MtE_MotorCar13-62m
    Wagon ( MtE_MotorCar13 MtE_MotorCar13-62m )
    Type ( Electric )

  Sound ( "MediumPitch_P01235_cab.sms" )
    Name ( "MtE Motor 13 [steel body]" "MtE Motor 13 [steel body] 6.2meter" )
    Description (

-----------------------------------------------------------------------------------------------------------------------------------------------------------
MtE_Motorcar14-62m.sd:

Shape ( MtE_MotorCar14.s MtE_MotorCar14-62m.s
	ESD_Detail_Level ( 0 )
	ESD_Software_DLev ( 3 )
	ESD_Alternative_Texture ( 0 )
	ESD_Bounding_Box ( -1.512000 0.023000 -9.600000 1.512000 4.250000 9.600000 )
)

-----------------------------------------------------------------------------------------------------------------------------------------------------------
MtE_MotorCar14-62m.eng:

Wagon ( MtE_MotorCar14 MtE_MotorCar14-62m
	Type ( Engine )
	WagonShape ( MtE_MotorCar14.s MtE_MotorCar14-62m.s )
 	PassengerCapacity ( 72.0 )
	Size  ( 3.01992m 4.22469m 19.7m )

Engine ( MtE_MotorCar14 MtE_MotorCar14-62m
    Wagon ( MtE_MotorCar14 MtE_MotorCar14-62m )
    Type ( Electric )

Sound ( "MediumPitch_P01235_cab.sms" )
Name ( "MtE Motor 14 [one panto/fwd]" "MtE Motor 14 [one panto/fwd] 6.2meter" )
Description (

-----------------------------------------------------------------------------------------------------------------------------------------------------------
MtE_Motorcar15-62m.sd:

Shape ( MtE_MotorCar15.s MtE_MotorCar15-62m.s
	ESD_Detail_Level ( 0 )
	ESD_Software_DLev ( 3 )
	ESD_Alternative_Texture ( 0 )
	ESD_Bounding_Box ( -1.512000 0.023000 -9.600000 1.512000 4.250000 9.600000 )
)

-----------------------------------------------------------------------------------------------------------------------------------------------------------
MtE_MotorCar15-62m.eng:

Wagon ( MtE_MotorCar15 MtE_MotorCar15-62m
	Type ( Engine )
	WagonShape ( MtE_MotorCar15.s MtE_MotorCar15-62m.s )
 	PassengerCapacity ( 72.0 )
	Size  ( 3.01992m 4.22469m 19.7m )

Engine ( MtE_MotorCar15 MtE_MotorCar15-62m
    Wagon ( MtE_MotorCar15 MtE_MotorCar15-62m )
    Type ( Electric )

    Sound ( "MediumPitch_P01235_cab.sms" )
    Name ( "MtE Motor 15 [one panto/rear]" "MtE Motor 15 [one panto/rear] 6.2meter" )
    Description (

-----------------------------------------------------------------------------------------------------------------------------------------------------------
MtE_MotorCombine16-62m.sd:

Shape ( MtE_MotorCombine16.s MtE_MotorCombine16-62m.s
	ESD_Detail_Level ( 0 )
	ESD_Software_DLev ( 3 )
	ESD_Alternative_Texture ( 0 )
	ESD_Bounding_Box ( -1.512000 0.023000 -9.600000 1.512000 4.250000 9.600000 )
)

-----------------------------------------------------------------------------------------------------------------------------------------------------------
MtE_MotorCombine16-62m.eng:

Wagon ( MtE_MotorCombine16 MtE_MotorCombine16-62m
	Type ( Engine )
	WagonShape ( MtE_MotorCombine16.s MtE_MotorCombine16-62m.s )
 	PassengerCapacity ( 40.0 )
	Size  ( 3.01992m 4.22469m 19.7m )

Engine ( MtE_MotorCombine16 MtE_MotorCombine16-62m
    Wagon ( MtE_MotorCombine16 MtE_MotorCombine16-62m )
    Type ( Electric )

  Sound ( "MediumPitch_P01235_cab.sms" )
    Name ( "MtE Motor Combine 16" "MtE Motor Combine 16 6.2meter" )
    Description (
-----------------------------------------------------------------------------------------------------------------------------------------------------------
MtE_MotorCombine17-62m.sd:

Shape ( MtE_MotorCombine17.s MtE_MotorCombine17-62m.s
	ESD_Detail_Level ( 0 )
	ESD_Software_DLev ( 3 )
	ESD_Alternative_Texture ( 0 )
	ESD_Bounding_Box ( -1.512000 0.023000 -9.600000 1.512000 4.250000 9.600000 )
)

-----------------------------------------------------------------------------------------------------------------------------------------------------------
MtE_MotorCombine17-62m.eng:

Wagon ( MtE_MotorCombine17 MtE_MotorCombine17-62m
	Type ( Engine )
	WagonShape ( MtE_MotorCombine17.s MtE_MotorCombine17-62m.s )
 	PassengerCapacity ( 40.0 )
	Size  ( 3.01992m 4.22469m 19.7m )

Engine ( MtE_MotorCombine17 MtE_MotorCombine17-62m
    Wagon ( MtE_MotorCombine17 MtE_MotorCombine17-62m )
    Type ( Electric )

    Sound ( "MediumPitch_P01235_cab.sms" )
    Name ( "MtE Motor Combine 17" "MtE Motor Combine 17 6.2meter" )
    Description (

-----------------------------------------------------------------------------------------------------------------------------------------------------------
MtE_MotorWorks11-62m.sd:

Shape ( MtE_MotorWorks11.s MtE_MotorWorks11-62m.s
	ESD_Detail_Level ( 0 )
	ESD_Software_DLev ( 3 )
	ESD_Alternative_Texture ( 0 )
	ESD_Bounding_Box ( -1.512000 0.023000 -9.600000 1.512000 4.250000 9.600000 )
)

-----------------------------------------------------------------------------------------------------------------------------------------------------------
MtE_MotorWorks11-62m.eng:

Wagon ( MtE_MotorWorks11 MtE_MotorWorks11-62m
	Type ( Engine )
	WagonShape ( MtE_MotorWorks11.s MtE_MotorWorks11-62m.s )
 	PassengerCapacity ( 6.0 )
	Size  ( 3.01992m 4.22469m 19.7m )

Engine ( MtE_MotorWorks11 MtE_MotorWorks11-62m
    Wagon ( MtE_MotorWorks11 MtE_MotorWorks11-62m )
    Type ( Electric )

    Sound ( "MediumPitch_CRS3L_cab.sms" )
    Name ( "MtE Motor Works 11" "MtE Motor Works 11 6.2meter" )
    Description (

-----------------------------------------------------------------------------------------------------------------------------------------------------------
Make copies of MtE_MotorCar41.s, MtE_MotorCar41.sd, MtE_MotorCar41.eng, MtE_MotorCar42.s (unit set up to run flipped at back of consist), MtE_MotorCar42.sd, MtE_MotorCar42.eng, MtE_MotorCar43.s (unit set up to run flipped at back of consist), MtE_MotorCar43.sd, MtE_MotorCar43.eng and name them MtE_MotorCar41-62m.s, MtE_MotorCar41-62m.sd, MtE_MotorCar41-62m.eng, MtE_MotorCar42-62m.s, MtE_MotorCar42-62m.sd, MtE_MotorCar42-62m.eng, MtE_MotorCar43-62m.s, MtE_MotorCar43-62m.sd, MtE_MotorCar43-62m.eng.

-----------------------------------------------------------------------------------------------------------------------------------------------------------
MtE_MotorCar41-62m.s, MtE_MotorCar42-62m.s, MtE_MotorCar43-62m.s:

	anim_node PantographBottom1A ( 
		controllers ( 1 
			tcb_rot ( 2 
				tcb_key ( 0 0 0 0 1 0 0 0 0 0 ) 
				tcb_key ( 1 -0.358368 -0.190809 0 0 0.93358 0.9816272 0 0 0 0 0 ) 
			) 
		) 
	) 
	anim_node PantographBottom1B ( 
		controllers ( 1 
			tcb_rot ( 2 
				tcb_key ( 0 -6.98132E-08 0 0 1 0 0 0 0 0 ) 
				tcb_key ( 1 -0.358368 -0.190809 0 0 -0.93358 -0.9816272 0 0 0 0 0 ) 
			) 
		) 
	) 
	anim_node PantographMiddle1A ( 
		controllers ( 2 
			tcb_rot ( 2 
				tcb_key ( 0 -4.01426E-07 0 0 1 0 0 0 0 0 ) 
				tcb_key ( 1 -0.313164 -0.190809 0 0 -0.949699 -0.9816272 0 0 0 0 0 ) 
			) 
			linear_pos ( 2 
				linear_key ( 0 0 0.237744 -2.46278 ) 
				linear_key ( 1 0 1.47828 0.93 -1.90805 -2.3 ) 
			) 
		) 
	) 
	anim_node PantographMiddle1B ( 
		controllers ( 2 
			tcb_rot ( 2 
				tcb_key ( 0 3.04616E-10 0.00436331 -6.98125E-08 0.99999 0 0 0 0 0 ) 
				tcb_key ( 1 -0.313164 -0.190809 0 0 0.949699 0.9816272 0 0 0 0 0 ) 
			) 
			linear_pos ( 2 
				linear_key ( 0 0 0.237744 2.46278 ) 
				linear_key ( 1 0 1.47828 0.93 1.90805 2.3 ) 
			) 
		) 
	) 
	anim_node PantographTop1A ( 
		controllers ( 1 
			linear_pos ( 2 
				linear_key ( 0 0 0.382219 0 ) 
				linear_key ( 1 0 3.05836 2.05836 0 ) 
			) 
		) 
	) 
	anim_node FMount ( 
		controllers ( 0 
		) 
	) 
	anim_node PantographBottom2A ( 
		controllers ( 1 
			tcb_rot ( 2 
				tcb_key ( 0 0 0 0 1 0 0 0 0 0 ) 
				tcb_key ( 1 -0.358368 -0.190809 0 0 0.93358 0.9816272 0 0 0 0 0 ) 
			) 
		) 
	) 
	anim_node PantographBottom2B ( 
		controllers ( 1 
			tcb_rot ( 2 
				tcb_key ( 0 -6.98132E-08 0 0 1 0 0 0 0 0 ) 
				tcb_key ( 1 -0.358368 -0.190809 0 0 -0.93358 -0.9816272 0 0 0 0 0 ) 
			) 
		) 
	) 
	anim_node PantographMiddle2A ( 
		controllers ( 2 
			tcb_rot ( 2 
				tcb_key ( 0 -4.01426E-07 0 0 1 0 0 0 0 0 ) 
				tcb_key ( 1 -0.313164 -0.190809 0 0 -0.949699 -0.9816272 0 0 0 0 0 ) 
			) 
			linear_pos ( 2 
				linear_key ( 0 0 0.237744 -2.46278 ) 
				linear_key ( 1 0 1.47828 0.93 -1.90805 -2.3 ) 
			) 
		) 
	) 
	anim_node PantographMiddle2B ( 
		controllers ( 2 
			tcb_rot ( 2 
				tcb_key ( 0 3.04616E-10 0.00436331 -6.98125E-08 0.99999 0 0 0 0 0 ) 
				tcb_key ( 1 -0.313164 -0.190809 0 0 0.949699 0.9816272 0 0 0 0 0 ) 
			) 
			linear_pos ( 2 
				linear_key ( 0 0 0.237744 2.46278 ) 
				linear_key ( 1 0 1.47828 0.93 1.90805 2.3 ) 
			) 
		) 
	) 
	anim_node PantographTop2A ( 
		controllers ( 1 
			linear_pos ( 2 
				linear_key ( 0 0 0.382219 0 ) 
				linear_key ( 1 0 3.05836 2.05836 0 ) 
			) 
		) 
	) 

-----------------------------------------------------------------------------------------------------------------------------------------------------------
MtE_MotorCar41-62m.sd:

Shape ( MtE_MotorCar41.s MtE_MotorCar41-62m.s
	ESD_Detail_Level ( 0 )
	ESD_Software_DLev ( 3 )
	ESD_Alternative_Texture ( 0 )
	ESD_Bounding_Box ( -1.463000 0.022300 -10.250000 1.463000 4.014000 10.250000 )
)
-----------------------------------------------------------------------------------------------------------------------------------------------------------
MtE_MotorCar41-62m.eng:

Wagon ( MtE_MotorCar41 MtE_MotorCar41-62m
	Type ( Engine )
	WagonShape ( MtE_MotorCar41.s MtE_MotorCar41-62m.s )
 	PassengerCapacity ( 82.0 )
	Size  ( 3.0063m 4.225m 20.9m )

Engine ( MtE_MotorCar41 MtE_MotorCar41-62m
    Wagon ( MtE_MotorCar41 MtE_MotorCar41-62m )
    Type ( Electric )

    Sound ( "HiPitch_CRS3L_cab.sms" )
    Name ( "MtE Motor 41 [panto 2 up]" "MtE Motor 41 [panto 2 up] 6.2meter" )
    Description (
-----------------------------------------------------------------------------------------------------------------------------------------------------------
MtE_MotorCar42-62m.sd:

Shape ( MtE_MotorCar42.s MtE_MotorCar42-62m.s
	ESD_Detail_Level ( 0 )
	ESD_Software_DLev ( 3 )
	ESD_Alternative_Texture ( 0 )
	ESD_Bounding_Box ( -1.463000 0.022300 -10.250000 1.463000 4.014000 10.250000 )
)

-----------------------------------------------------------------------------------------------------------------------------------------------------------
MtE_MotorCar42-62m.eng:

Wagon ( MtE_MotorCar42 MtE_MotorCar42-62m
	Type ( Engine )
	WagonShape ( MtE_MotorCar42.s MtE_MotorCar42-62m.s )
 	PassengerCapacity ( 82.0 )
	Size  ( 3.0063m 4.225m 20.9m )

Engine ( MtE_MotorCar42 MtE_MotorCar42-62m
    Wagon ( MtE_MotorCar42 MtE_MotorCar42-62m )
    Type ( Electric )

    Sound ( "HiPitch_CRS3L_cab.sms" )
    Name ( "MtE Motor 42 [panto 1 up]" "MtE Motor 42 [panto 1 up] 6.2meter" )
    Description (
 -----------------------------------------------------------------------------------------------------------------------------------------------------------
MtE_MotorCar43-62m.sd:

Shape ( MtE_MotorCar43.s MtE_MotorCar43-62m.s
	ESD_Detail_Level ( 0 )
	ESD_Software_DLev ( 3 )
	ESD_Alternative_Texture ( 0 )
	ESD_Bounding_Box ( -1.463000 0.022300 -10.250000 1.463000 4.014000 10.250000 )
)

-----------------------------------------------------------------------------------------------------------------------------------------------------------
MtE_MotorCar43-62m.eng:

Wagon ( MtE_MotorCar43 MtE_MotorCar43-62m
	Type ( Engine )
	WagonShape ( MtE_MotorCar43.s MtE_MotorCar43-62m.s )
 	PassengerCapacity ( 82.0 )
	Size  ( 3.0063m 4.225m 20.9m )

Engine ( MtE_MotorCar43 MtE_MotorCar43-62m
    Wagon ( MtE_MotorCar43 MtE_MotorCar43-62m )
    Type ( Electric )

    Sound ( "HiPitch_CRS3L_cab.sms" )
    Name ( "MtE Motor 43 [panto 1 up]" "MtE Motor 43 [panto 1 up] 6.2meter" )
    Description (
 -----------------------------------------------------------------------------------------------------------------------------------------------------------
Make copies of MtE_P1_6.s, MtE_P1_6.sd, MtE_P1_6.eng, MtE_P1_7.s, MtE_P1_7.sd, MtE_P1_7.eng and name them MtE_P1_6-62m.s, MtE_P1_6-62m.sd, MtE_P1_6-62m.eng, MtE_P1_7-62m.s, MtE_P1_7-62m.sd, MtE_P1_7-62m.eng.

-----------------------------------------------------------------------------------------------------------------------------------------------------------
MtE_P1_6-62m.s, MtE_P1_7-62m.s:

	anim_node PantographBottom1A ( 
		controllers ( 1 
			tcb_rot ( 2 
				tcb_key ( 0 0 0 0 1 0 0 0 0 0 ) 
				tcb_key ( 8 -0.333807 -0.1564345 0 0 0.942641 0.9876883 0 0 0 0 0 ) 
			) 
		) 
	) 
	anim_node PantographMiddle1B ( 
		controllers ( 2 
			tcb_rot ( 2 
				tcb_key ( 0 0 0 0 1 0 0 0 0 0 ) 
				tcb_key ( 8 -0.267238 -0.1564345 0 0 0.96363 0.9876883 0 0 0 0 0 ) 
			) 
			linear_pos ( 2 
				linear_key ( 0 0 0.19812 2.50698 ) 
				linear_key ( 8 0 1.35941 0.78 1.9873 2.35 ) 
			) 
		) 
	) 
	anim_node PantographMiddle1A ( 
		controllers ( 2 
			tcb_rot ( 2 
				tcb_key ( 0 0 0 0 1 0 0 0 0 0 ) 
				tcb_key ( 8 -0.267238 -0.1564345 0 0 -0.96363 -0.9876883 0 0 0 0 0 ) 
			) 
			linear_pos ( 2 
				linear_key ( 0 0 0.19812 -2.50698 ) 
				linear_key ( 8 0 1.35941 0.78 -1.9873 -2.35 ) 
			) 
		) 
	) 
	anim_node PantographTop1A ( 
		controllers ( 1 
			linear_pos ( 2 
				linear_key ( 0 0 0.42672 0 ) 
				linear_key ( 8 0 2.8194 1.8194 0 ) 
			) 
		) 
	) 
	anim_node FPantographBottom1A ( 
		controllers ( 0 
		) 
	) 
	anim_node PantographBottom1B ( 
		controllers ( 1 
			tcb_rot ( 2 
				tcb_key ( 0 0 0 0 1 0 0 0 0 0 ) 
				tcb_key ( 8 -0.333807 -0.1564345 0 0 -0.942642 -0.9876883 0 0 0 0 0 ) 
			) 
		) 
	) 

-----------------------------------------------------------------------------------------------------------------------------------------------------------
MtE_P1_6-62m.sd:

Shape ( MtE_P1_6.s MtE_P1_6-62m.s
	ESD_Detail_Level ( 0 )
	ESD_Software_DLev ( 3 )
	ESD_Alternative_Texture ( 0 )
	ESD_Bounding_Box ( -1.600000 0.023000 -11.850000 1.600000 4.530000 11.850000 )
)

-----------------------------------------------------------------------------------------------------------------------------------------------------------
MtE_P1_6-62m.eng:

Wagon ( MtE_P1_6 MtE_P1_6-62m
	Type ( Engine )
	WagonShape ( MtE_P1_6.s MtE_P1_6-62m.s )
	PassengerCapacity ( 1 )
	Size  ( 3.20106m 3.95042m 24.0m )

Engine ( MtE_P1_6 MtE_P1_6-62m
    Wagon ( MtE_P1_6 MtE_P1_6-62m )
    Type ( Electric )

    Sound ( "LowPitch_CRS3L_cab.sms" )
    Name ( "MtE P1 Motor 6 [green/panto 2]" "MtE P1 Motor 6 [green/panto 2] 6.2meter" )
    Description (

-----------------------------------------------------------------------------------------------------------------------------------------------------------
MtE_P1_7-62m.sd:

Shape ( MtE_P1_7.s MtE_P1_7-62m.s
	ESD_Detail_Level ( 0 )
	ESD_Software_DLev ( 3 )
	ESD_Alternative_Texture ( 0 )
	ESD_Bounding_Box ( -1.600000 0.023000 -11.850000 1.600000 4.530000 11.850000 )
)

-----------------------------------------------------------------------------------------------------------------------------------------------------------
MtE_P1_7-62m.eng:

Wagon ( MtE_P1_7 MtE_P1_7-62m
	Type ( Engine )
	WagonShape ( MtE_P1_7.s MtE_P1_7-62m.s )
	PassengerCapacity ( 1 )
	Size  ( 3.20106m 3.95042m 24.0m )

Engine ( MtE_P1_7 MtE_P1_7-62m
    Wagon ( MtE_P1_7 MtE_P1_7-62m )
    Type ( Electric )

    Sound ( "LowPitch_CRS3L_cab.sms" )
    Name ( "MtE P1 Motor 7 [panto 2]" "MtE P1 Motor 7 [panto 2] 6.2meter" )
    Description (

-----------------------------------------------------------------------------------------------------------------------------------------------------------
Make copies of MtE_P1_8.s, MtE_P1_8.sd, MtE_P1_8.eng, MtE_P1_9.s, MtE_P1_9.sd, MtE_P1_9.eng and name them MtE_P1_8-62m.s, MtE_P1_8-62m.sd, MtE_P1_8-62m.eng, MtE_P1_9-62m.s, MtE_P1_9-62m.sd, MtE_P1_9-62m.eng.

-----------------------------------------------------------------------------------------------------------------------------------------------------------
MtE_P1_8-62m.s, MtE_P1_9-62m.s:

	anim_node PantographBottom1A ( 
		controllers ( 1 
			tcb_rot ( 2 
				tcb_key ( 0 0 0 0 1 0 0 0 0 0 ) 
				tcb_key ( 8 -0.333807 -0.1564345 0 0 0.942641 0.9876883 0 0 0 0 0 ) 
			) 
		) 
	) 
	anim_node PantographMiddle1B ( 
		controllers ( 2 
			tcb_rot ( 2 
				tcb_key ( 0 0 0 0 1 0 0 0 0 0 ) 
				tcb_key ( 8 -0.267238 -0.1564345 0 0 0.96363 0.9876883 0 0 0 0 0 ) 
			) 
			linear_pos ( 2 
				linear_key ( 0 0 0.19812 2.50698 ) 
				linear_key ( 8 0 1.35941 0.78 1.9873 2.35 ) 
			) 
		) 
	) 
	anim_node PantographMiddle1A ( 
		controllers ( 2 
			tcb_rot ( 2 
				tcb_key ( 0 0 0 0 1 0 0 0 0 0 ) 
				tcb_key ( 8 -0.267238 -0.1564345 0 0 -0.96363 -0.9876883 0 0 0 0 0 ) 
			) 
			linear_pos ( 2 
				linear_key ( 0 0 0.19812 -2.50698 ) 
				linear_key ( 8 0 1.35941 0.78 -1.9873 -2.35 ) 
			) 
		) 
	) 
	anim_node PantographTop1A ( 
		controllers ( 1 
			linear_pos ( 2 
				linear_key ( 0 0 0.42672 0 ) 
				linear_key ( 8 0 2.8194 1.8194 0 ) 
			) 
		) 
	) 
	anim_node RPantographBottom1A ( 
		controllers ( 0 
		) 
	) 
	anim_node PantographBottom1B ( 
		controllers ( 1 
			tcb_rot ( 2 
				tcb_key ( 0 0 0 0 1 0 0 0 0 0 ) 
				tcb_key ( 8 -0.333807 -0.1564345 0 0 -0.942642 -0.9876883 0 0 0 0 0 ) 
			) 
		) 
	) 

-----------------------------------------------------------------------------------------------------------------------------------------------------------
MtE_P1_8-62m.sd:

Shape ( MtE_P1_8.s MtE_P1_8-62m.s
	ESD_Detail_Level ( 0 )
	ESD_Software_DLev ( 3 )
	ESD_Alternative_Texture ( 0 )
	ESD_Bounding_Box ( -1.600000 0.023000 -11.85000 1.600000 4.530000 11.850000 )
)

-----------------------------------------------------------------------------------------------------------------------------------------------------------
MtE_P1_8-62m.eng:

Wagon ( MtE_P1_8 MtE_P1_8-62m
	Type ( Engine )
	WagonShape ( MtE_P1_8.s MtE_P1_8-62m )
	PassengerCapacity ( 1 )
	Size  ( 3.20106m 3.95042m 24.0m )

Engine ( MtE_P1_8 MtE_P1_8-62m
    Wagon ( MtE_P1_8 MtE_P1_8-62m )
    Type ( Electric )

	Sound ( "LowPitch_CRS3L_cab.sms" )
	Name ( "MtE P1 Motor 8 [panto 1]" "MtE P1 Motor 8 [panto 1] 6.2meter" )
	Description (

-----------------------------------------------------------------------------------------------------------------------------------------------------------
MtE_P1_9-62m.sd:

Shape ( MtE_P1_8.s MtE_P1_8-62m.s
	ESD_Detail_Level ( 0 )
	ESD_Software_DLev ( 3 )
	ESD_Alternative_Texture ( 0 )
	ESD_Bounding_Box ( -1.600000 0.023000 -11.85000 1.600000 4.530000 11.850000 )
)

-----------------------------------------------------------------------------------------------------------------------------------------------------------
MtE_P1_9-62m.eng:

Wagon ( MtE_P1_9 MtE_P1_9-62m
	Type ( Engine )
	WagonShape ( MtE_P1_9.s MtE_P1_9-62m )
	PassengerCapacity ( 1 )
	Size  ( 3.20106m 3.95042m 24.0m )

Engine ( MtE_P1_9 MtE_P1_9-62m
    Wagon ( MtE_P1_9 MtE_P1_9-62m )
    Type ( Electric )

	Sound ( "LowPitch_CRS3L_cab.sms" )
	Name ( "MtE P1 Motor 9 [panto 1]" "MtE P1 Motor 9 [panto 1] 6.2meter" )
	Description (

-----------------------------------------------------------------------------------------------------------------------------------------------------------
Make copies of MtE_P5_3.s, MtE_P5_3.sd, MtE_P5_3.eng, MtE_P5_4.s, MtE_P5_4.sd, MtE_P5_4.eng and name them MtE_P5_3-62m.s, MtE_P5_3-62m.sd, MtE_P5_3-62m.eng, MtE_P5_4-62m.s, MtE_P5_4-62m.sd, MtE_P5_4-62m.eng respectively.

-----------------------------------------------------------------------------------------------------------------------------------------------------------
MtE_P5_3-62m.s, MtE_P5_4-62m.s:

	anim_node PantographBottom2A ( 
		controllers ( 1 
			tcb_rot ( 2 
				tcb_key ( 0 0 0 0 1 0 0 0 0 0 ) 
				tcb_key ( 8 -0.333807 -0.1650476 0 0 0.942641 0.9862856 0 0 0 0 0 ) 
			) 
		) 
	) 
	anim_node PantographBottom2B ( 
		controllers ( 1 
			tcb_rot ( 2 
				tcb_key ( 0 0 0 0 1 0 0 0 0 0 ) 
				tcb_key ( 8 -0.333807 -0.1650476 0 0 -0.942642 -0.9862856 0 0 0 0 0 ) 
			) 
		) 
	) 
	anim_node PantographMiddle2A ( 
		controllers ( 2 
			tcb_rot ( 2 
				tcb_key ( 0 0 0 0 1 0 0 0 0 0 ) 
				tcb_key ( 8 -0.284015 -0.1650476 0 0 -0.95882 -0.9862856 0 0 0 0 0 ) 
			) 
			linear_pos ( 2 
				linear_key ( 0 0 0.21336 -2.50698 ) 
				linear_key ( 8 0 1.35941 0.82 -1.9873 -2.35 ) 
			) 
		) 
	) 
	anim_node PantographMiddle2B ( 
		controllers ( 2 
			tcb_rot ( 2 
				tcb_key ( 0 0 0 0 1 0 0 0 0 0 ) 
				tcb_key ( 8 -0.284015 -0.1650476 0 0 0.95882 0.9862856 0 0 0 0 0 ) 
			) 
			linear_pos ( 2 
				linear_key ( 0 0 0.21336 2.50698 ) 
				linear_key ( 8 0 1.35941 0.82 1.9873 2.35 ) 
			) 
		) 
	) 
	anim_node PantographTop2A ( 
		controllers ( 1 
			linear_pos ( 2 
				linear_key ( 0 0 0.44196 0 ) 
				linear_key ( 8 0 2.88036 1.88036 0 ) 
			) 
		) 
	) 
	anim_node Mount ( 
		controllers ( 0 
		) 
	) 
	anim_node PantographBottom1A ( 
		controllers ( 1 
			tcb_rot ( 2 
				tcb_key ( 0 0 0 0 1 0 0 0 0 0 ) 
				tcb_key ( 8 -0.333807 -0.1650476 0 0 0.942641 0.9862856 0 0 0 0 0 ) 
			) 
		) 
	) 
	anim_node PantographBottom1B ( 
		controllers ( 1 
			tcb_rot ( 2 
				tcb_key ( 0 0 0 0 1 0 0 0 0 0 ) 
				tcb_key ( 8 -0.333807 -0.1650476 0 0 -0.942642 -0.9862856 0 0 0 0 0 ) 
			) 
		) 
	) 
	anim_node PantographMiddle1B ( 
		controllers ( 2 
			tcb_rot ( 2 
				tcb_key ( 0 0 0 0 1 0 0 0 0 0 ) 
				tcb_key ( 8 -0.284015 -0.1650476 0 0 0.95882 -0.9862856  0 0 0 0 0 ) 
			) 
			linear_pos ( 2 
				linear_key ( 0 0 0.21336 2.50698 ) 
				linear_key ( 8 0 1.35941 0.82 1.9873 2.35 ) 
			) 
		) 
	) 
	anim_node PantographMiddle1A ( 
		controllers ( 2 
			tcb_rot ( 2 
				tcb_key ( 0 0 0 0 1 0 0 0 0 0 ) 
				tcb_key ( 8 -0.284015 -0.1650476 0 0 -0.95882 -0.9862856 0 0 0 0 0 ) 
			) 
			linear_pos ( 2 
				linear_key ( 0 0 0.21336 -2.50698 ) 
				linear_key ( 8 0 1.35941 0.82 -1.9873 -2.35 ) 
			) 
		) 
	) 
	anim_node PantographTop1A ( 
		controllers ( 1 
			linear_pos ( 2 
				linear_key ( 0 0 0.44196 0 ) 
				linear_key ( 8 0 2.88036 1.88036 0 ) 
			) 
		) 
	) 

-----------------------------------------------------------------------------------------------------------------------------------------------------------
MtE_P5_3-62m.sd:

Shape ( MtE_P5_3.s MtE_P5_3-62m.s
	ESD_Detail_Level ( 0 )
	ESD_Software_DLev ( 3 )
	ESD_Alternative_Texture ( 0 )
	ESD_Bounding_Box ( -1.60 0.02 -9.35 1.60 4.48 9.35 )
)

-----------------------------------------------------------------------------------------------------------------------------------------------------------
MtE_P5_3-62m.eng:

Wagon ( MtE_P5_3 MtE_P5_3-62m
	Type ( Engine )
	WagonShape ( MtE_P5_3.s MtE_P5_3-62m.s )
	PassengerCapacity ( 1 )
	Size  ( 3.20106m 4.49827m 19.15m )

Engine ( MtE_P5_3 MtE_P5_3-62m
    Wagon ( MtE_P5_3 MtE_P5_3-62m )
    Type ( Electric )

  Sound ( "MediumPitch_CRS3L_cab.sms" )
    Name ( "MtE P5 Motor 3 [Panto 2]" "MtE P5 Motor 3 [Panto 2] 6.2meter" )
    Description (

-----------------------------------------------------------------------------------------------------------------------------------------------------------
MtE_P5_4-62m.sd:

Shape ( MtE_P5_4.s MtE_P5_4-62m.s
	ESD_Detail_Level ( 0 )
	ESD_Software_DLev ( 3 )
	ESD_Alternative_Texture ( 0 )
	ESD_Bounding_Box ( -1.60 0.02 -9.35 1.60 4.48 9.35 )
)

-----------------------------------------------------------------------------------------------------------------------------------------------------------
MtE_P5_4-62m.eng:

Wagon ( MtE_P5_4 MtE_P5_4-62m
	Type ( Engine )
	WagonShape ( MtE_P5_4.s MtE_P5_4-62m.s )
	PassengerCapacity ( 1 )
	Size  ( 3.20106m 4.49827m 19.15m )

Engine ( MtE_P5_4 MtE_P5_4-62m
    Wagon ( MtE_P5_4 MtE_P5_4-62m )
    Type ( Electric )

    Sound ( "MediumPitch_CRS3L_cab.sms" )
    Name ( "MtE P5 Motor 4 [Panto 1]" "MtE P5 Motor 4 [Panto 1] 6.2m" )
    Description (

-----------------------------------------------------------------------------------------------------------------------------------------------------------